jGfx - CubeTex_SyncMRT

# CubeTex_SyncMRT

CubeTex_SyncMRT pCubeTex, pCubeTexB, pCubeTexC, pCubeTexD, CameraID

## Description

Renders to up to 4 CubeTexures simultaneously using the specified DBPro camera. The camera must have a target image whos resolution is equal to or greater than the CubeTex's resolution. The first CubeTex's view data will be used when rendering.

## Parameters

pCubeTex | INTEGER | First CubeTex render target
pCubeTexB | INTEGER | Second CubeTex render target
pCubeTexC | INTEGER | Third CubeTex render target, specify 0 if not needed
pCubeTexD | INTEGER | Fourth CubeTex render target, specify 0 if not needed
CameraID | INTEGER | ID of the camera to use when rendering

CubeTex Commands
jGfx Command Index
jGfx Main